{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Parameters","TP Summaries"],"not_rendered":{"charts":0,"images":12,"macros":1,"external_links":0,"defined_names":32,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":true,"merged":[[12,5,14,5],[15,5,16,5],[24,4,24,5]]}
[]
[]
[]
[]
[]
[null,"notes for combining toolpaths"]
[]
[null,"1st tp"]
[null,null,"deleted","G0X0.000Y0.000",null,"will leave spindle above last hole"]
[null,null,null,"M2"]
[]
[null,"2nd tp"]
[null,null,"deleted","T1","tool 1","established in 1st tp"]
[null,null,null,"G17","arcs in xy plane"]
[null,null,null,"G21","units-mm"]
[null,null,null,"G90","absolute values","established at end of 1st tp"]
[null,null,null,"G0Z20.000"]
[null,null,null,"G0X0.000Y0.000",null,"not necessary, can go directly to first hole upon resume"]
[null,null,null,"S10000M3",null,"established in 1st tp (and not controllable on my router anyway)"]
[]
[null,null,"added"]
[null,null,null,"G0Y228.000","move x-axis back out of the way. Will use maxY in VBA"]
[null,null,null,"M9","coolant off","turns off router thru IOT"]
[null,null,null,"M0","pause"]
[null,null,null,null,"reposition workpiece, then resume"]
[null,null,null,"M8","coolant on"]

{"sheet":"Parameters","index":1,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[[21,1,21,2],[3,1,3,8],[13,3,14,3],[17,1,17,8],[19,1,19,2],[0,1,0,8],[1,2,1,3],[2,2,2,3],[2,5,2,8],[20,1,20,2]]}
[null,"Line Bore Gcode Generator"]
[null,"Project Name:","Green Way Place"]
[null,"Toolpath Filename:","LineBoreTP",null,"-##","(a 2 digit index number will be appended\neach toolpath using this name)"]
[null,"• Parameters"]
[]
[null,"Holes:","Diameter:",5,"Spacing:",32,"Depth:",10,1]
[null,"Panel:","Thickness:",0.75,"Width:",4,"Length:",24,25.4]
[null,null,null,null,"This is a cabinet ",null," side panel"]
[null,"Backsets:","Front:",35,"Back:",20,1]
[null,"                                                             (Remember to consider Face Frames & Back Rabbets)"]
[null,"Number of Columns of Holes:",2]
[null,"Index Holes from:","bottom","end of Panel"]
[null,"                                             (Remember to consider Cabinet Top & Bottom Panel Thicknesses)"]
[null,"Start Distance from Index End:",2,25.4]
[null,"Minimum Stop Distance from other End:",1.5]
[]
[]
[null,"• Machine Settings"]
[]
[null,"Max Cutting Length of Machine:",null,9,25.4]
[null,"Minimum Safe Z:\n(for moving up a column):",null,5,1]
[null,"High Clearance Z:\n(for big, rapid moves across work surface)",null,20,1]
[null,"Drilling:","Spindle:",10000,"RPM"]
[null,null,"Plunge Rate:",3000,1,"/minute"]

{"sheet":"TP Summaries","index":2,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,2]]}
[{"$f":"CONCATENATE(\"Linebore TP Parameters: \", name_p)","v":"Linebore TP Parameters: Green Way Place"}]
["→→→   PANEL SET-UP IN ALL CASES:  FRONT EDGE @ X = 0,  INDEX END @ Y = 0   ←←←"]